# Uses of Package
com.h3c.util.ip

- Packages that use com.h3c.util.ip
  Package | Description
  --- | ---
  com.h3c.of.common | Code shared by the OpenFlow Controller and Mock OpenFlow Switch implementations.
  com.h3c.of.ctl | Public API for the OpenFlow Controller.
  com.h3c.of.json | JSON factory and codecs for Openflow structures.
  com.h3c.of.lib.dt | A set of classes representing data values used in the OpenFlow protocol.
  com.h3c.of.lib.instr | Representations of OpenFlow Protocol Instructions and Actions.
  com.h3c.of.lib.match | Representations of OpenFlow Protocol Match Structures.
  com.h3c.of.lib.mp | Representations of OpenFlow Protocol Multipart Message bodies.
  com.h3c.of.lib.msg | Representations of OpenFlow Protocol Messages.
  com.h3c.of.sw | Provides mock implementations of OpenFlow switches.
  com.h3c.sdn.adm | Definitions of the domain model and services specific to the Administrator tier of the VCF Controller.
  com.h3c.sdn.adm.backup |
  com.h3c.sdn.adm.dao.model | Model POJOs implementations used to persist and retrieve information applicable at the Administrator tier of the SDN Controller.
  com.h3c.sdn.adm.role | ...
  com.h3c.sdn.adm.system | Definitions of services pertaining to the SDN Controller system and its collaborators.
  com.h3c.sdn.api | Definitions of services for driving outbound external communications for interacting with peers and integrating with other external applications, e.g.
  com.h3c.sdn.common | Definitions of general services applicable to multiple tiers of the SDN Controller.
  com.h3c.sdn.ctlAddrManager |
  com.h3c.sdn.diag | Definitions of the path diagnostic service.
  com.h3c.sdn.hostManager |
  com.h3c.sdn.linkdisco | Definitions of the services provided by the Link Discovery Application.
  com.h3c.sdn.misc | Miscellaneous SDN-specific utilities and auxiliaries for use as part of implementations in either tier; entities provided within cannot not be used as part of the mutual interface between the tiers however.
  com.h3c.sdn.misc.net |
  com.h3c.sdn.nodemgr | Definitions of the services provided by the Node Manager Application.
  com.h3c.sdn.region | ...
  com.h3c.sdn.system | Definitions of the domain model pertaining to the SDN Controller system.
  com.h3c.sdn.teamconfig | Team configuration information.
  com.h3c.sdn.teamcs | ...
  com.h3c.sdn.topology | Definitions of the interfaces provided by the Topology Services Application.
  com.h3c.util.ip |
  com.h3c.util.pkt |
  com.h3c.util.snmp |
  com.h3c.util.snmp.command |

- Classes in com.h3c.util.ip used by com.h3c.of.common
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.of.ctl
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).
  PortNumber Represents a port number (unsigned 16-bit).

- Classes in com.h3c.util.ip used by com.h3c.of.json
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  EthernetType Represents an Ethernet frame type.
  ICMPv4Type Represents an ICMPv4 message type.
  ICMPv6Type Represents an ICMPv6 message type.
  IpAddress Represents an IP address (either IPv4 or IPv6).
  IpProtocol Represents an IP Protocol.
  MacAddress Represents a MAC address.
  PortNumber Represents a port number (unsigned 16-bit).

- Classes in com.h3c.util.ip used by com.h3c.of.lib.dt
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.
  PortNumber Represents a port number (unsigned 16-bit).
  U16Id A base class for unsigned 16-bit identifiers.
  U32Id A base class for unsigned 32-bit identifiers.
  U8Id A base class for unsigned 8-bit identifiers.
  UnsignedId Forms the basis of datatype classes represented by unsigned values.
  UnsignedIntBasedId A base class for unsigned identifiers with an integer payload.
  UnsignedLongBasedId A base class for unsigned identifiers with a long payload.

- Classes in com.h3c.util.ip used by com.h3c.of.lib.instr
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  EthernetType Represents an Ethernet frame type.
  ICMPv4Type Represents an ICMPv4 message type.
  ICMPv6Type Represents an ICMPv6 message type.
  IpAddress Represents an IP address (either IPv4 or IPv6).
  IpProtocol Represents an IP Protocol.
  MacAddress Represents a MAC address.
  PortNumber Represents a port number (unsigned 16-bit).

- Classes in com.h3c.util.ip used by com.h3c.of.lib.match
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  EthernetType Represents an Ethernet frame type.
  ICMPv4Type Represents an ICMPv4 message type.
  ICMPv6Type Represents an ICMPv6 message type.
  IpAddress Represents an IP address (either IPv4 or IPv6).
  IpProtocol Represents an IP Protocol.
  MacAddress Represents a MAC address.
  PortNumber Represents a port number (unsigned 16-bit).

- Classes in com.h3c.util.ip used by com.h3c.of.lib.mp
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).

- Classes in com.h3c.util.ip used by com.h3c.of.lib.msg
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  MacAddress Represents a MAC address.
  PortNumber Represents a port number (unsigned 16-bit).

- Classes in com.h3c.util.ip used by com.h3c.of.sw
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacPrefix Represents a MAC address prefix; that is to say, the top N bytes of the address are fixed (where N is 1 to 5) and the remaining bytes are unspecified.

- Classes in com.h3c.util.ip used by com.h3c.sdn.adm
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.adm.backup
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.adm.dao.model
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.adm.role
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.adm.system
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.api
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.common
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.ctlAddrManager
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.diag
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).

- Classes in com.h3c.util.ip used by com.h3c.sdn.hostManager
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.linkdisco
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).

- Classes in com.h3c.util.ip used by com.h3c.sdn.misc
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.misc.net
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.nodemgr
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.region
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.sdn.system
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.teamconfig
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).

- Classes in com.h3c.util.ip used by com.h3c.sdn.teamcs
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).

- Classes in com.h3c.util.ip used by com.h3c.sdn.topology
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).

- Classes in com.h3c.util.ip used by com.h3c.util.ip
  Class and Description
  AlphaNumericName Represents an alpha-numeric name.
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  DnsName Represents a DNS name.
  EthernetType Represents an Ethernet frame type.
  ICMPv4Type Represents an ICMPv4 message type.
  ICMPv6Type Represents an ICMPv6 message type.
  IfType IANA Interface types.
  IpAddress Represents an IP address (either IPv4 or IPv6).
  IpAddress.AddressClass Specifies the IP address class.
  IpAddress.Family Specifies the IP address families.
  IpDnsPair Links together an `IpAddress` and a `DnsName` as a pair.
  IpProtocol Represents an IP Protocol.
  IpRange Represents a range of IP addresses.
  MacAddress Represents a MAC address.
  MacAddress.Format Designates the different MAC address string formats available.
  MacPrefix Represents a MAC address prefix; that is to say, the top N bytes of the address are fixed (where N is 1 to 5) and the remaining bytes are unspecified.
  MacRange Represents a range of MAC addresses.
  PartialSubnet Represents a `Subnet` that has one or more `IpRange`s associated with it that narrow the scope of the subnet (hence "partial").
  PortNumber Represents a port number (unsigned 16-bit).
  Subnet Represents a subnet.
  SubnetMask Represents a subnet mask (either IPv4 or IPv6).
  TcpUdpPort Represents a tcp/udp port.
  TcpUdpPortPair Represents a pair of ports defined by a source `IpAddress` and `TcpUdpPort` and a destination `IpAddress` and `TcpUdpPort`.
  U16Id A base class for unsigned 16-bit identifiers.
  U32Id A base class for unsigned 32-bit identifiers.
  UnsignedId Forms the basis of datatype classes represented by unsigned values.
  UnsignedIntBasedId A base class for unsigned identifiers with an integer payload.
  UnsignedLongBasedId A base class for unsigned identifiers with a long payload.

- Classes in com.h3c.util.ip used by com.h3c.util.pkt
  Class and Description
  BigPortNumber Represents a switch port number (unsigned 32-bit).
  EthernetType Represents an Ethernet frame type.
  ICMPv4Type Represents an ICMPv4 message type.
  ICMPv6Type Represents an ICMPv6 message type.
  IpAddress Represents an IP address (either IPv4 or IPv6).
  IpProtocol Represents an IP Protocol.
  MacAddress Represents a MAC address.
  PortNumber Represents a port number (unsigned 16-bit).
  TcpUdpPort Represents a tcp/udp port.

- Classes in com.h3c.util.ip used by com.h3c.util.snmp
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

- Classes in com.h3c.util.ip used by com.h3c.util.snmp.command
  Class and Description
  IpAddress Represents an IP address (either IPv4 or IPv6).
  MacAddress Represents a MAC address.

Copyright © 2014. All Rights Reserved.